



                                MAD! PRESENTS...



                         THE ABC'S OF PAYPHONES PART 1



The information presented in this file is for entertainment purposes

only.  The authors of this file take no responsibility for any of its

contents.



The following text file is for AT&T & GTE payphones from 1982-1985. some

things are different on gte phones, so additions are included for them.



Section 1:The coin slot



For every 5 cents you put in a phone, a sound is made.  After you put

the coins in the slot, they pass through a  totalizer which counts them.

They then collect in a hopper.  To empty out the hopper, all you have to

do is activate the coin relay.  Payphones sometimes hold $100 or more.

To activate the relay place 5 cents in the phone.  Stick a magnet up the

coin slot about 5 inches.  Now remove the front panel of the phone. You

will see a series of wires.  Cut the red and green wires.  Now in the

front of the panel you will see three screws. Touch the green wire to

the third screw.  Better have a hat ready, because alot of change is

gonna come flooding out.  Isn't this fun?



Section 2:free credits



If you have a friend jn germany you need to call this section's for you.

One of the cheap things about pay phones is they depend on tones to tell

them you inserted money.  Well if you have a red box these tones are

easily duplicated, but i want to show you how do it without boxes in

this file.  Now Some things you need are... A set of screwdrivers.  You will

need both philips and flathead.  Now open the front panel of the phone and cut

the red and green wires.  Take the cover off the top of the phone and insert 5

cents.  You should hear nothing.  Find a green wire coming from the coin slot

down to the hopper.  Disconnect that wire.  Now take off the case and you will

see a small switch.  Move the switch.  This sets the totalizer backwards 1.

Now put the hopper cover back on and reconnect the wire. Back to the front

panel.  Feel to the right of the two screws.  You should feel 4 jumpers.

1 of the jumpers should be disconnected.  Reconnect it. Now cut the top

jumper. You should hear a loud pop.  Now touch the green wire to the second

screw.  You will hear the sound of twenty five cents being inserted.  You now

have 30 cents credit.  Repeat as many times as you need. Now reconnect the

green wire and dial your number.



GTE Notes:

The green wire will be white. The red one will be blue.  The totalizer

is located at the bottem of the front panel.



In part 2 we will show you how to take the payphone apart, and how to

take one home.


